Gaius Hospital Classic XL ja 2XL -mallipohjien tarvikeluettelo

**Hospital basin**

Hospital basins are made of a durable and antimicrobial cast marble. The Hospital basin has fixed rails on both sides to support standing and ease approach. The rounded front edge combined with the side rails, with antimicrobial elastomeric coating, form a uniform support rail. Load-bearing capacity of rails 160 kg. Mounting hardware sold separately. The basin without overflow is a special order product, with a 6 to 8 week delivery time.

**Dimensions**: W800 x D800 mm

**With overflow**6502GAM Hospital basin, white, grey elastomer rail, with overflow, antimicrobial

6500RAM Hospital basin, white, red elastomer rail, with overflow, antimicrobial

**Without overflow (special order)**6519GAM Hospital basin, white, grey elastomer rail, without overflow, antimicrobial

6517RAM Hospital basin, white, red elastomer rail, without overflow, antimicrobial

**Hospital basin height adjustment options**
Mounting hardware sold separately.

6232W Height adjustment rails, 3 per basin

6237N Crank height adjustment
6511N Electric height adjustment
6216-Z Height adjustment rails mounting hardware
6216-Z Electric and crank height adjustment mounting hardware

**Hospital basin height adjustment accessories**

X300 Telescope pipe for water trap (height adjustment rails)
992600 Accordion pipe (electric and crank height adjustment)
6223 90º wall mounting for water trap

**Bide basin**

The Luna bide basin is made of white antimicrobial cast marble. Right- and left-handed basins available, classified by the location of the faucet. Without overflow. A fixed water trap and mounting hardware are included.

**Dimensions**: W390 x H90 x D270 mm

6509AM Bide basin, right-handed (faucet on right)

6510AM Bide basin, left-handed (faucet on left)

**Paper towel – or dispenser cabinets**

Cabinets have a white moisture resistant frame made of 16 mm melamine, with grey accent strips. The doors are made of high-pressure laminate with additional grey accent strips along the edges to promote spatial recognition. Orientation of the doors is changeable.

**Dimensions**: W300 x H900 x D135 mm

6326 Paper towel cabinet, paper towel dispenser above, shelf below, 2 doors

6327 Paper towel cabinet, paper towel dispenser below, shelf above, 1 tall door

6320 HH Dispenser cabinet, includes 2 Dispenso Pac units and paper towel dispenser, 2 doors

**Gaius shower seat, height adjustable**

Gaius shower seats are made of integral plastic, which makes them easy to clean and comfortable to use. All metal parts are antimicrobial stainless steel or aluminium, painted with white epoxy-paint. Customizable with hand rails. Height adjustment range 300 mm. Height adjustment via hex key. Load-bearing capacity 250 kg.

17372W Shower seat, grey, height adjustable

**Gaius hand rails for the Gaius shower seat**

Hand rails for the shower seat model 17372W. The white frame is antimicrobial steel or aluminum, with elastomeric non-slip handles. Hand rails can be moved individually.

6522N Hand rails, grey

6520 Hand rails, red

1770 Hand rails, grey

**Regal support rails, height adjustable, 3 pieces**

The antimicrobial and height adjustable Regal support rails are painted white, with elastomeric coating to provide a non-slip grip. The adjustment lever allows for stepless height adjustment. Rails are equipped with hinges that aid with folding, and keeping the rails in an upright position. Height adjustment range is 200 mm.
Rail diameter is 30 x 33 mm. Hardware is painted steel, with plastic cover plates. Load-bearing capacity 250 kg at mid-height, and side-ways 225 kg. Yellow rails are special order products, with a 12 week delivery time for a minimum order of 25 pieces.

**Dimensions**: Length 800 mm / 900 mm

20106G Regal support rail, height adjustable, length 800 mm, grey, antimicrobial

20106R Regal support rail, height adjustable, length 800 mm, red, antimicrobial

20106Y Regal support rail, height adjustable, length 800 mm, yellow, antimicrobial

20204G Regal support rail, height adjustable, length 900 mm, grey, antimicrobial

20204R Regal support rail, height adjustable, length 900 mm, red, antimicrobial

20204Y Regal support rail, height adjustable, length 900 mm, yellow, antimicrobial

**Regal support rail accessories**

1721 Toilet paper dispenser, stainless steel

1764N Hand shower holder, jointed, stainless steel

20120 Chest support bar

**Modular hand rail**

Modular hand rails have a slim, oval shape, which allows for a firm grip. The rail frame is aluminum, with a non-slip, antimicrobial Soft Touch -paint cover. Additional hardware is polymer. Mounting hardware included. Load-bearing capacity 225 kg. Yellow rails are a special order product, with a 6 to 8 week delivery time for a minimum order of 50 pieces.

**Dimensions:** Rail diameter 30 x 33 mm

16366W Modular L support rail, 800 + 600 mm 90°, white, antimicrobial

16366G Modular L support rail, 800 + 600 mm 90°, grey, antimicrobial

16366R Modular L support rail, 800 + 600 mm 90°, red, antimicrobial

16366Y Modular L support rail, 800 + 600 mm 90°, yellow, antimicrobial

16399W Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, white, antimicrobial

16399G Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, grey, antimicrobial

16399R Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, red, antimicrobial

16399Y Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, yellow, antimicrobial

**Modular shower rail accessory**

16501 Adjustment bar for the shower head holder, long

**Solo E rail**

The ergonomic slim oval shape of the rail, coupled with the antimicrobial aluminum frame yields a safe and hygienic hand rail. Rail diameter 30 x 33 mm.

1677W Solo E rail, 500 mm, white, antimicrobial

1677G Solo E rail, 500 mm, grey, antimicrobial

1677R Solo E rail, 500 mm, red, antimicrobial

**Mirror or mirror cabinet**

6530 Corner mirror, W500 x H1000 mm, mounted via special corner piece, rounded edges

6532 Senior mirror cabinet, W600 x H800 x D130 mm, white, melamine shelves, double sided mirrored doors,
two socket electrical outlet inside

6533 Corner mirror cabinet, W400 x H900 mm, solid base, two movable shelves, laminate frame

**Lights**

9551 LED light, W415 mm, 12W, 1200 lm, IP44, 3000K/4000K/6000K

6110 Gaius mirror light, W600 mm, 1 x 24 W, electronic ballast, IP44

9207 Gaius Universal light, W600 mm, 2 x 55 W, IP44

**Toilet brush holder**

RST Line, wall mounted, lacquered, suitable for different brushes, brush not included.

1309 Toilet brush holder, stainless steel, W105 x H250 x D100 mm

1309WAM Toilet brush holder, stainless steel / white, W105 x H250 x D100 mm, antimicrobial

335 Toilet brush, 400 mm, white

340 Toilet brush, 530 mm, white

**Soap trays**

1921 Large soap tray, shallow, W290 x H50 x D130 mm, chromed

1928 Detergent basket for support rail, W295 x H150 x D130 mm + 200 mm cuffs, chromed

**Hook**

1907 Double hook for clothes, steel / white, 2 pieces

**TOOLFLEX rack**

1509 Walking stick, crutch, or mop holder, white, holds diameter 20-30 mm, 2 pieces

**Liquid soap dispensers for disposable packages**

1226 Dispenso pac, wall mounted, elbow operated, 2 pieces

1241LAM vas Dispenso pac, wall mounted, stainless steel, elbow operated, lockable, lacquered, antimicrobial, 2 pieces

**Dustbin or trash bag holder**

1320LAM Dustbin, RST Line, without lid, 30 L, lacquered, W335 x H450 x D185 mm, antimicrobial

1882N Steel wire basket without lid, 30 L, stainless steel, W340 x H500 x D255 mm

1882-1LAM Lid for basket 1882N, antimicrobial

**Mounting hardware**

Mounting hardware for shower seat and support rails sold separately.

Alternatives to the products included in the model floorplan available.

For more information, consult our website or sales associates at **korpinen@korpinen.com**.