Gaius Original Classic XL and 2XL model floorplan catalogue

**Original basin**

Original basins are made of a durable and antimicrobial cast marble. A Korpinen classic, the Original basin has fixed rails in front to support standing and ease approach. A toilet paper dispenser, wall brackets, and fixed water trap are included with the basin. Mounting hardware sold separately. Load-bearing capacity 230 kg. Yellow rails for the Original basin are a special order product, with a 12 week delivery time for a minimum order of 12 pieces.

**Dimensions:** W1000 x D500 mm (D575 mm with rail)

**With overflow (without overflow is special order)**

6202WAM Original basin, right-handed, white, white rail, with overflow, antimicrobial

6202GAM Original basin, right-handed, white, grey rail, with overflow, antimicrobial

6202RAM Original basin, right-handed, white, red rail, with overflow, antimicrobial  
6202YAM Original basin, right-handed, white, yellow rail, with overflow, antimicrobial

6203WAM Original basin, left-handed, white, white rail, with overflow, antimicrobial

6203GAM Original basin, left-handed, white, grey rail, with overflow, antimicrobial

6203RAM Original basin, left-handed, white, red rail, with overflow, antimicrobial  
6203YAM Original basin, left-handed, white, yellow rail, with overflow, antimicrobial

**Original basin, rounded rail ends**

**With overflow (without overflow is special order)**

6202WCAM Original basin, right-handed, white, white rail, with overflow, antimicrobial

6202GCAM Original basin, right-handed, white, grey rail, with overflow, antimicrobial

6202RCAM Original basin, right-handed, white, red rail, with overflow, antimicrobial   
6202YCAM Original basin, right-handed, white, yellow rail, with overflow, antimicrobial

6203WCAM Original basin, left-handed, white, white rail, with overflow, antimicrobial

6203GCAM Original basin, left-handed, white, grey rail, with overflow, antimicrobial

6203RCAM Original basin, left-handed, white, red rail, with overflow, antimicrobial   
6203YCAM Original basin, left-handed, white, yellow rail, with overflow, antimicrobial

**Original basin height adjustment options**  
Mounting hardware sold separately.

6232W Height adjustment rails, 2 pieces

6236N Crank height adjustment system   
6513N Electric height adjustment

20064-Z Height adjustment rail mounting hardware, 2 per basin

6218-Z Crank height adjustment mounting hardware

6218-Z Electric height adjustment mounting hardware

**Original basin height adjustment accessories**   
X300 Telescope pipe for water trap (height adjustment rails)  
992600 Accordion pipe (electric and crank height adjustment)   
6223 90º wall mounting for water trap

**Gaius storage cabinet**

Gaius cabinets have a white moisture resistant frame made of 16 mm melamine. The wall mounted cabinets ease cleaning in humid bathroom conditions. The doors are made of high-pressure laminate with additional grey accent strips along the edges to promote spatial recognition. Orientation of the doors is changeable.

**Dimensions**: W400 x H1800 x D500 mm

6300W/G/R/Y Storage cabinet, includes 2 fixed shelves, a pull-out laundry basket and drawer, fixed enclosing for an electrical outlet (sockets not included). White/grey/red/yellow rail.

**Paper towel – or dispenser cabinets**

Cabinets have a white moisture resistant frame made of 16 mm melamine, with grey accent strips. The doors are made of high-pressure laminate with additional grey accent strips along the edges to promote spatial recognition. Orientation of the doors is changeable.

**Dimensions**: W300 x H900 x D135 mm

6326 Paper towel cabinet, paper towel dispenser above, shelf below, 2 doors

6327 Paper towel cabinet, paper towel dispenser below, shelf above, 1 tall door

6320 HH Dispenser cabinet, includes 2 Dispenso Pac units and paper towel dispenser, 2 doors

**Gaius shower seat, height adjustable**

Gaius shower seats are made of integral plastic, which makes them easy to clean and comfortable to use. All metal parts are antimicrobial stainless steel or aluminium, painted with white epoxy-paint. Customizable with hand rails. Height adjustment range 300 mm. Height adjustment via hex key. Load-bearing capacity 250 kg.

17372W Shower seat, grey, height adjustable

**Gaius hand rails for the Gaius shower seat**

Hand rails for the shower seat model 17372W. The white frame is antimicrobial steel or aluminum, with elastomeric non-slip handles. Hand rails can be moved individually.

6522N Hand rails, grey

6520 Hand rails, red

1770 Hand rails, grey

**Stay 15 support rail, height adjustable, 2 pieces**

Finnish-made Stay support rails are made of antimicrobial, white epoxy-painted steel, with elastomeric gripping surfaces. Additional hardware is aluminum. Rail diameter 22 mm. Height adjustment range 200 mm. Mounting hardware sold separately. Yellow support rails are a special order product, with a 12 week delivery time for a minimum order of 45 pieces.

10115GW Stay 15 support rail, 920 mm, grey

10115RW Stay 15 support rail, 920 mm, red

10115YW Stay 15 support rail, 920 mm, yellow

**Stay support rail accessories**

1756 Toilet paper holder

1759 Alarm button holder

1768N Hand shower holder

20120 Chest support bar

1901 Hook for the chest support bar

20064-Z Mounting hardware

**Modular hand rail**

Modular hand rails have a slim, oval shape, which allows for a firm grip. The rail frame is aluminum, with a non-slip, antimicrobial Soft Touch -paint cover. Additional hardware is polymer. Mounting hardware included. Load-bearing capacity 225 kg. Yellow rails are a special order product, with a 6 to 8 week delivery time for a minimum order of 50 pieces.

**Dimensions:** Rail diameter 30 x 33 mm

16366W Modular L support rail, 800 + 600 mm 90°, white, antimicrobial

16366G Modular L support rail, 800 + 600 mm 90°, grey, antimicrobial

16366R Modular L support rail, 800 + 600 mm 90°, red, antimicrobial

16366Y Modular L support rail, 800 + 600 mm 90°, yellow, antimicrobial

16399W Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, white, antimicrobial

16399G Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, grey, antimicrobial

16399R Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, red, antimicrobial

16399Y Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, yellow, antimicrobial

**Modular shower rail accessory**

16501 Adjustment bar for the shower head holder, long

**Mirror**

6101 Gaius mirror, W600 x H900 mm, rounded edges, mounting hardware aluminum

**Lights**

9552 LED light, mounting to wall or cabinet, W590 mm, 12 W, 1200 lm, IP44

6110 Gaius mirror light, W600 mm, 1 x 24 W, electronic ballast, IP44

**Toilet brushes and brush holders**

RST Line, wall mounted, lacquered, suitable for different brushes, brush not included.

1309 Toilet brush holder, stainless steel, W105 x H250 x D100 mm

1309WAM Toilet brush holder, stainless steel / white, W105 x H250 x D100 mm, antimicrobial

13091 Toilet brush holder with detachable cup

335 Toilet brush, 400 mm, white

340 Toilet brush, 530 mm, white

**Soap trays**

1921 Large soap tray, shallow, W290 x H50 x D130 mm, chromed

6077.0 Soap tray, deep, W200 x H110 x D90 mm, chromed

**Hook**

1907 Double hook for clothes, steel / white, 2 pieces

**Dustbin**

1321LAM RST Line, stainless steel, 30L, with lid, W335 x H450 mm, lacquered, antimicrobial

**TOOLFLEX rack**

1509 Walking stick, crutch, or mop holder, white, holds diameter 20-30 mm

**Mounting hardware**

Mounting hardware for shower seat and support rails sold separately.

Alternatives to the products included in the model floorplan available.

For more information, consult our website or sales associates at **korpinen@korpinen.com**.