Gaius Hospital Sense XL and 2XL model floorplan catalogue

**Sense corner basin**

Gaius Sense Corner basins are made of a durable and antimicrobial composite material. The basin is seamless, with fixed rails in front to support standing and ease approach. A toilet paper dispenser, a white pop-up drain plug, fixed water trap, and mounting hardware are included with the basin. Load-bearing capacity 400 kg.

**Dimensions:** W840 x D840 mm

**With overflow**

65001WAM Sense corner basin, white, with overflow, antimicrobial

65001GAM Sense corner basin, white, grey accent strip, with overflow, antimicrobial

65001RAM Sense corner basin, white, red accent strip, with overflow, antimicrobial

**Without overflow**

65000WAM Sense corner basin, white, without overflow, antimicrobial

65000GAM Sense corner basin, white, grey accent strip, without overflow, antimicrobial65000RAM Sense corner basin, white, red accent strip, without overflow, antimicrobial

**Sense corner basin height adjustment options**
Mounting hardware sold separately.

6234W Height adjustment rails
6244N Crank height adjustment system
65111 Electric height adjustment

20064-Z Height adjustment rail mounting hardware, 3 per basin

6216-Z Electric and crank height adjustment mounting hardware

**Sense corner basin height adjustment accessories**
X300 Telescope pipe for water trap (height adjustment rails)
992600 Accordion pipe (electric and crank height adjustment)
6223 90º wall mounting for water trap

**Bide basin**

The Luna bide basin is made of white antimicrobial cast marble. Right- and left-handed basins available, classified by the location of the faucet. Without overflow. A fixed water trap and mounting hardware are included.

**Dimensions**: W390 x H90 x D270 mm

6509AM Bide basin, right-handed (faucet on right)

6510AM Bide basin, left-handed (faucet on left)

**Paper towel – or dispenser cabinets**

Cabinets have a white moisture resistant frame made of 16 mm melamine, with grey accent strips. The doors are made of high-pressure laminate with additional grey accent strips along the edges to promote spatial recognition. Orientation of the doors is changeable.

**Dimensions**: W300 x H900 x D135 mm

6326 Paper towel cabinet, paper towel dispenser above, shelf below, 2 doors

6327 Paper towel cabinet, paper towel dispenser below, shelf above, 1 tall door

6320 HH Dispenser cabinet, includes 2 Dispenso Pac units and paper towel dispenser, 2 doors

**Sense shower seat,** **height adjustable**

The antimicrobial, height adjustable Sense shower seat suits locations with multiple different users. The seat is mounted to a single height adjustment rail, by which it can be adjusted without tools in two steps. Adjustment range is 300 mm without additional hand rails. The seat can also be customized to include an arm and back rest.

Hinges aid with folding, and keeping the seat in an upright position. The seat is made of soft integral plastic, with a white frame. Load-bearing capacity 400 kg. Yellow seats are special order products, with a 12 week delivery time for a minimum order of 110 pieces.

**Dimensions**: W430 x H600 x D510 mm (D210 mm when folded up)

17412G Sense shower seat, height adjustable, grey, antimicrobial

17412R Sense shower seat, height adjustable, red, antimicrobial

17412Y Sense shower seat, height adjustable, yellow, antimicrobial

17413G Sense shower seat with hole, height adjustable, grey, antimicrobial

17413R Sense shower seat with hole, height adjustable, red, antimicrobial

17413Y Sense shower seat with hole, height adjustable, yellow, antimicrobial

**Sense hand and back support for the Sense shower seat**

Combined hand and back support makes it easier to sit down. Hand rails can be moved individually. Rails have an elastomeric coating which provides a non-slip grip. Antimicrobial. Yellow hand rails are a special order product, with a 12 week delivery time for a minimum of 110 pieces.

**Dimensions**: W590 x H130 x D535 mm (elastomeric coating for W280, back support pad W195 x H145 mm)

17414G Sense hand and back support, grey, antimicrobial
17414R Sense hand and back support, red, antimicrobial
17414Y Sense hand and back support, yellow, antimicrobial

**Regal support rails, height adjustable, 3 pieces**

The antimicrobial and height adjustable Regal support rails are painted white, with elastomeric coating to provide a non-slip grip. The adjustment lever allows for stepless height adjustment. Rails are equipped with hinges that aid with folding, and keeping the rails in an upright position. Height adjustment range is 200 mm.
Rail diameter is 30 x 33 mm. Hardware is painted steel, with plastic cover plates. Load-bearing capacity 250 kg at mid-height, and side-ways 225 kg. Yellow rails are special order products, with a 12 week delivery time for a minimum order of 25 pieces.

**Dimensions**: Length 800 mm / 900 mm

20106G Regal support rail, height adjustable, length 800 mm, grey, antimicrobial

20106R Regal support rail, height adjustable, length 800 mm, red, antimicrobial

20106Y Regal support rail, height adjustable, length 800 mm, yellow, antimicrobial

20204G Regal support rail, height adjustable, length 900 mm, grey, antimicrobial

20204R Regal support rail, height adjustable, length 900 mm, red, antimicrobial

20204Y Regal support rail, height adjustable, length 900 mm, yellow, antimicrobial

**Regal support rail accessories**

1721 Toilet paper dispenser, stainless steel

1764N Hand shower holder, jointed, stainless steel

20120 Chest support bar

**Solo hand rail**

The seamless, antimicrobial design of the Solo hand rail, coupled with the slim, oval shape of the bar provides a firm grip. The rail Ø 33 x 30 mm. Load-bearing capacity 225 kg. Mounting hardware included.

16802W Solo hand rail, 800 mm, white, antimicrobial

16802G Solo hand rail, 800 mm, grey, antimicrobial

16802R Solo hand rail, 800 mm, red, antimicrobial

16804W Solo hand rail, 1200 mm, shower support, 1 shower head holder, white, antimicrobial

16804G Solo hand rail, 1200 mm, shower support, 1 shower head holder, grey, antimicrobial

16804R Solo hand rail, 1200 mm, shower support, 1 shower head holder, red, antimicrobial

**Solo E rail**

The ergonomic slim oval shape of the rail, coupled with the antimicrobial aluminum frame yields a safe and hygienic hand rail. Rail diameter 30 x 33 mm.

1677W Solo E rail, 500 mm, white, antimicrobial

1677G Solo E rail, 500 mm, grey, antimicrobial

1677R Solo E rail, 500 mm, red, antimicrobial

**Mirror or mirror cabinet**

6530 Corner mirror, W500 x H1000 mm, mounted via special corner piece, rounded edges

6532 Senior mirror cabinet, W600 x H800 x D130 mm, white, melamine shelves, double sided mirrored doors,
two socket electrical outlet inside

6533 Corner mirror cabinet, W400 x H900 mm, solid base, two movable shelves, laminate frame

**Light**

9551 LED light, W415 mm, 12W, 1200 lm, IP44, 3000K/4000K/6000K

**Toilet brush holder**

RST Line, wall mounted, lacquered, suitable for different brushes, brush not included.

1309 Toilet brush holder, stainless steel, W105 x H250 x D100 mm

1309WAM Toilet brush holder, stainless steel / white, W105 x H250 x D100 mm, antimicrobial

335 Toilet brush, 400 mm, white

340 Toilet brush, 530 mm, white

**Soap trays**

1921 Large soap tray, shallow, W290 x H50 x D130 mm, chromed

1928 Detergent basket for support rail, W295 x H150 x D130 mm + 200 mm cuffs, chromed

**Hook**

1907 Double hook for clothes, steel / white, 2 pieces

**TOOLFLEX rack**

1509 Walking stick, crutch, or mop holder, white, holds diameter 20-30 mm, 2 pieces

**Liquid soap dispensers for disposable packages**

1226 Dispenso pac, wall mounted, elbow operated, 2 pieces

1241LAM vas Dispenso pac, wall mounted, stainless steel, elbow operated, lockable, lacquered, antimicrobial, 2 pieces

**Dustbin or trash bag holder**

1320LAM Dustbin, RST Line, without lid, 30 L, lacquered, W335 x H450 x D185 mm, antimicrobial

1882N Steel wire basket without lid, 30 L, stainless steel, W340 x H500 x D255 mm

1882-1LAM Lid for basket 1882N, antimicrobial

**Mounting hardware**

Mounting hardware for shower seat and support rails sold separately.

Alternatives to the products included in the model floorplan available.

For more information, consult our website or sales associates at **korpinen@korpinen.com**.