Gaius Original Sense XL and 2XL model floorplan catalogue

**Sense basin**

Gaius Sense basins are made of a durable and antimicrobial composite material. The basin is seamless, with fixed rails in front to support standing and ease approach. A toilet paper dispenser, a white pop-up drain plug, fixed water trap, and mounting hardware are included with the basin. Load-bearing capacity 400 kg.

**Dimensions**: W900 x D576 mm

**With overflow**62023WAM Sense basin, right-handed, white, with overflow, antimicrobial
62023GAM Sense basin, right-handed, white, grey accent strip, with overflow, antimicrobial

62023RAM Sense basin, right-handed, white, red accent stip, with overflow, antimicrobial

62034WAM Sense basin, left-handed, white, with overflow, antimicrobial

62034GAM Sense basin, left-handed, white, grey accent strip, with overflow, antimicrobial

62034RAM Sense basin, left-handed, white, red accent strip, with overflow, antimicrobial

 **Without overflow**

62022WAM Sense basin, right-handed, white, without overflow, antimicrobial

62022GAM Sense basin, right-handed, white, grey accent strip, without overflow, antimicrobial

62022RAM Sense basin, right-handed, white, red accent strip, without overflow, antimicrobial

62033WAM Sense basin, left-handed, white, without overflow, antimicrobial

62033GAM Sense basin, left-handed, white, grey accent strip, without overflow, antimicrobial

62033RAM Sense basin, left-handed, white, red accent strip, without overflow, antimicrobial

**Sense basin height adjustment options**

Mounting hardware sold separately.

6233W Height adjustment rails

6243 Crank height adjustment system

65133 Electric height adjustment
20064-Z Height adjustment rail mounting hardware, 2 per basin
6218-Z Electric and crank height adjustment mounting hardware
**Sense basin height adjustment accessories**
X300 Telescope pipe for water trap (height adjustment rails)
992600 Accordion pipe (electric and crank height adjustment)
6223 90º wall mounting for water trap

**Gaius storage cabinet**

Gaius cabinets have a white moisture resistant frame made of 16 mm melamine. The wall mounted cabinets ease cleaning in humid bathroom conditions. The doors are made of high-pressure laminate with additional grey accent strips along the edges to promote spatial recognition. Orientation of the doors is changeable.

**Dimensions**: W400 x H1800 x D500 mm

6309 Storage cabinet, two fixed shelves above, fixed enclosing for an electrical outlet (sockets not included).
Pull-out laundry basket and drawer below.

6313 Storage cabinet, 2 doors, 2 fixed shelves above, fixed enclosing for an electrical outlet (sockets not included).
2 fixed shelves below.

16801W/G/R Solo support rail, 600 mm, vertically mounted to side of storage cabinet 6313. Grey, red, or white.

**Paper towel – or dispenser cabinets**

Cabinets have a white moisture resistant frame made of 16 mm melamine, with grey accent strips. The doors are made of high-pressure laminate with additional grey accent strips along the edges to promote spatial recognition. Orientation of the doors is changeable.

**Dimensions**: W300 x H900 x D135 mm

6326 Paper towel cabinet, paper towel dispenser above, shelf below, 2 doors

6327 Paper towel cabinet, paper towel dispenser below, shelf above, 1 tall door

6320 HH Dispenser cabinet, includes 2 Dispenso Pac units and paper towel dispenser, 2 doors

**Sense shower seat,** **height adjustable**

The antimicrobial, height adjustable Sense shower seat suits locations with multiple different users. The seat is mounted to a single height adjustment rail, by which it can be adjusted without tools in two steps. Adjustment range is 300 mm without additional hand rails. The seat can also be customized to include an arm and back rest.

Hinges aid with folding, and keeping the seat in an upright position. The seat is made of soft integral plastic, with a white frame. Load-bearing capacity 400 kg. Yellow seats are special order products, with a 12 week delivery time for a minimum order of 110 pieces.

**Dimensions**: W430 x H600 x D510 mm (D210 mm when folded up)

17412G Sense shower seat, height adjustable, grey, antimicrobial

17412R Sense shower seat, height adjustable, red, antimicrobial

17412Y Sense shower seat, height adjustable, yellow, antimicrobial

17413G Sense shower seat with hole, height adjustable, grey, antimicrobial

17413R Sense shower seat with hole, height adjustable, red, antimicrobial

17413Y Sense shower seat with hole, height adjustable, yellow, antimicrobial

**Sense hand and back support for the Sense shower seat**

Combined hand and back support makes it easier to sit down. Hand rails can be moved individually. Rails have an elastomeric coating which provides a non-slip grip. Antimicrobial. Yellow hand rails are a special order product, with a 12 week delivery time for a minimum of 110 pieces.

**Dimensions**: W590 x H130 x D535 mm (elastomeric coating for W280, back support pad W195 x H145 mm)

17414G Sense hand and back support, grey, antimicrobial
17414R Sense hand and back support, red, antimicrobial
17414Y Sense hand and back support, yellow, antimicrobial

**Regal support rails, height adjustable, 2 pieces**

The antimicrobial and height adjustable Regal support rails are painted white, with elastomeric coating to provide a non-slip grip. The adjustment lever allows for stepless height adjustment. Rails are equipped with hinges that aid with folding, and keeping the rails in an upright position. Height adjustment range is 200 mm.
Rail diameter is 30 x 33 mm. Hardware is painted steel, with plastic cover plates. Load-bearing capacity 250 kg at mid-height, and side-ways 225 kg. Yellow rails are special order products, with a 12 week delivery time for a minimum order of 25 pieces.

**Dimensions**: Length 900 mm

20204G Regal support rail, height adjustable, length 900 mm, grey, antimicrobial

20204R Regal support rail, height adjustable, length 900 mm, red, antimicrobial

20204Y Regal support rail, height adjustable, length 900 mm, yellow, antimicrobial

**Regal support rail accessories**

1721 Toilet paper dispenser, stainless steel

1764N Hand shower holder, jointed, stainless steel

20120 Chest support bar

**Modular hand rails**

Modular hand rails have a slim, oval shape, which allows for a firm grip. The rail frame is aluminum, with a non-slip, antimicrobial Soft Touch -paint cover. Additional hardware is polymer. Mounting hardware included. Load-bearing capacity 225 kg. Yellow rails are a special order product, with a 6 to 8 week delivery time for a minimum order of 50 pieces.

**Dimensions:** Rail diameter 30 x 33 mm

16366W Modular L support rail, 800 + 600 mm 90°, white, antimicrobial

16366G Modular L support rail, 800 + 600 mm 90°, grey, antimicrobial

16366R Modular L support rail, 800 + 600 mm 90°, red, antimicrobial

16366Y Modular L support rail, 800 + 600 mm 90°, yellow, antimicrobial

16399W Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, white, antimicrobial

16399G Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, grey, antimicrobial

16399R Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, red, antimicrobial

16399Y Modular shower rail, 450 + 1200 mm 90° + 1 shower head holder, yellow, antimicrobial

**Modular shower rail accessory**

16501 Adjustment bar for the shower head holder, long

**Mirror**

6101 Gaius mirror, W600 x H900 mm, rounded edges, mounting hardware aluminum

**Lights**

9552 LED light, mounting to wall or cabinet, W590 mm, 12 W, 1200 lm, IP44

6110 Gaius mirror light, W600 mm, 1 x 24 W, electronic ballast, IP44

**Toilet brushes and brush holders**

RST Line, wall mounted, lacquered, suitable for different brushes, brush not included.

1309 Toilet brush holder, stainless steel, W105 x H250 x D100 mm

1309WAM Toilet brush holder, stainless steel / white, W105 x H250 x D100 mm, antimicrobial

13091 Toilet brush holder with detachable cup

335 Toilet brush, 400 mm, white

340 Toilet brush, 530 mm, white

**Soap trays**

1921 Large soap tray, shallow, W290 x H50 x D130 mm, chromed

6077.0 Soap tray, deep, W200 x H110 x D90 mm, chromed

**Hook**

1907 Double hook for clothes, steel / white, 2 pieces

**TOOLFLEX rack**

1509 Walking stick, crutch, or mop holder, white, holds diameter 20-30 mm, 2 pieces

**Mounting hardware**

Mounting hardware for shower seat and support rails sold separately.

Alternatives to the products included in the model floorplan available.

For more information, consult our website or sales associates at **korpinen@korpinen.com**.